smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.14 (AF)
Device Model:     ST1000DM003-9YN162
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: CC82
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Wed Feb 10 19:06:49 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     254 (maximum performance)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  584) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 113) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x3085)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   119   097   006    -    206942056
  3 Spin_Up_Time            PO----   097   096   000    -    0
  4 Start_Stop_Count        -O--CK   097   097   020    -    3381
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    24
  7 Seek_Error_Rate         POSR--   080   060   030    -    103644078
  9 Power_On_Hours          -O--CK   095   095   000    -    4990
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   098   098   020    -    2378
183 Runtime_Bad_Block       -O--CK   093   093   000    -    7
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   063   063   000    -    37
188 Command_Timeout         -O--CK   100   099   000    -    1 1 3
189 High_Fly_Writes         -O-RCK   071   071   000    -    29
190 Airflow_Temperature_Cel -O---K   067   053   045    -    33 (Min/Max 18/33)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    1103
193 Load_Cycle_Count        -O--CK   091   091   000    -    19476
194 Temperature_Celsius     -O---K   033   047   000    -    33 (0 10 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   164   000    -    775
240 Head_Flying_Hours       ------   100   253   000    -    4112h+39m+13.976s
241 Total_LBAs_Written      ------   100   253   000    -    89029320685996
242 Total_LBAs_Read         ------   100   253   000    -    213839389328802
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS      20  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    5067  Device vendor specific log
0xbd       GPL     VS     512  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 34 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 34 [13] occurred at disk power-on lifetime: 4039 hours (168 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 9d 58 00 00  Error: UNC at LBA = 0x16909d58 = 378576216

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 16 90 9d 40 e0 00     02:22:31.197  READ DMA EXT
  25 00 00 01 00 00 00 16 90 9c 40 e0 00     02:22:31.196  READ DMA EXT
  25 00 00 01 00 00 00 16 90 9b 40 e0 00     02:22:31.195  READ DMA EXT
  35 00 00 01 00 00 00 49 a8 3a 50 e0 00     02:22:31.195  WRITE DMA EXT
  35 00 00 01 00 00 00 49 a8 39 50 e0 00     02:22:31.194  WRITE DMA EXT

Error 33 [12] occurred at disk power-on lifetime: 4036 hours (168 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 16 90 aa 50 e0 00     00:08:35.216  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a9 50 e0 00     00:08:35.215  READ DMA EXT
  25 00 00 01 00 00 00 13 53 27 40 e0 00     00:08:35.213  READ DMA EXT
  25 00 00 01 00 00 00 13 53 26 40 e0 00     00:08:35.198  READ DMA EXT
  25 00 00 00 88 00 00 0b 27 b7 c8 e0 00     00:08:35.197  READ DMA EXT

Error 32 [11] occurred at disk power-on lifetime: 4036 hours (168 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 16 90 aa e8 e0 00     00:08:09.212  READ DMA EXT
  25 00 00 01 00 00 00 16 8b 01 40 e0 00     00:08:09.210  READ DMA EXT
  25 00 00 01 00 00 00 16 8b 00 40 e0 00     00:08:09.193  READ DMA EXT
  25 00 00 01 00 00 00 13 4d 81 49 e0 00     00:08:09.191  READ DMA EXT
  25 00 00 01 00 00 00 13 4d 80 49 e0 00     00:08:09.191  READ DMA EXT

Error 31 [10] occurred at disk power-on lifetime: 4036 hours (168 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 16 90 aa 2c e0 00     00:07:34.098  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a9 2c e0 00     00:07:34.096  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a8 2c e0 00     00:07:34.096  READ DMA EXT
  25 00 00 00 81 00 00 13 44 6a 4d e0 00     00:07:34.095  READ DMA EXT
  25 00 00 01 00 00 00 13 44 69 4d e0 00     00:07:34.095  READ DMA EXT

Error 30 [9] occurred at disk power-on lifetime: 4034 hours (168 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 16 90 aa e8 e0 00     07:22:08.355  READ DMA EXT
  25 00 00 01 00 00 00 12 46 e7 70 e0 00     07:22:08.353  READ DMA EXT
  25 00 00 01 00 00 00 12 46 e6 70 e0 00     07:22:08.347  READ DMA EXT
  25 00 00 01 00 00 00 11 d5 86 e5 e0 00     07:22:08.346  READ DMA EXT
  25 00 00 01 00 00 00 11 d5 85 e5 e0 00     07:22:08.340  READ DMA EXT

Error 29 [8] occurred at disk power-on lifetime: 4034 hours (168 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 16 90 a9 21 e0 00     07:21:17.755  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a8 21 e0 00     07:21:17.737  READ DMA EXT
  25 00 00 00 88 00 00 12 3d e3 58 e0 00     07:21:17.736  READ DMA EXT
  25 00 00 01 00 00 00 12 3d e2 58 e0 00     07:21:17.735  READ DMA EXT
  25 00 00 01 00 00 00 12 3d e1 58 e0 00     07:21:17.735  READ DMA EXT

Error 28 [7] occurred at disk power-on lifetime: 4019 hours (167 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 01 00 00 16 90 aa e8 e0 00     05:28:42.234  READ DMA EXT
  25 00 00 01 00 00 00 4b 72 9e 03 e0 00     05:28:42.232  READ DMA EXT
  25 00 00 01 00 00 00 4b 72 9d 03 e0 00     05:28:42.232  READ DMA EXT
  25 00 00 00 01 00 00 16 90 aa e7 e0 00     05:28:42.232  READ DMA EXT
  25 00 00 01 00 00 00 4b 72 9c 03 e0 00     05:28:42.231  READ DMA EXT

Error 27 [6] occurred at disk power-on lifetime: 4019 hours (167 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 16 90 aa e8 00 00  Error: UNC at LBA = 0x1690aae8 = 378579688

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 00 16 90 aa 68 e0 00     05:28:38.211  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a9 68 e0 00     05:28:38.209  READ DMA EXT
  25 00 00 01 00 00 00 16 90 a8 68 e0 00     05:28:38.209  READ DMA EXT
  25 00 00 00 81 00 00 4b 6e 67 cf e0 00     05:28:38.208  READ DMA EXT
  25 00 00 01 00 00 00 4b 6e 66 cf e0 00     05:28:38.208  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    32 Celsius
Power Cycle Min/Max Temperature:     18/32 Celsius
Lifetime    Min/Max Temperature:     10/47 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            7  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



