smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Phison Driven OEM SSDs
Device Model:     SATA SSD
Serial Number:    --
Firmware Version: SBFM61.5
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-4 (minor revision not indicated)
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Thu Jul 28 20:14:31 2022 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(65535) seconds.
Offline data collection
capabilities: 			 (0x79) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  30) minutes.
Conveyance self-test routine
recommended polling time: 	 (   6) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   050    -    0
  9 Power_On_Hours          -O--C-   100   100   000    -    289
 12 Power_Cycle_Count       -O--C-   100   100   000    -    236
168 SATA_Phy_Error_Count    -O--C-   100   100   000    -    0
170 Bad_Blk_Ct_Erl/Lat      PO----   100   100   010    -    0/113
173 MaxAvgErase_Ct          -O--C-   100   100   000    -    26 (Average 25)
192 Unsafe_Shutdown_Count   -O--C-   100   100   000    -    72
194 Temperature_Celsius     PO---K   067   067   000    -    33 (Min/Max 33/33)
218 CRC_Error_Count         PO-R--   100   100   050    -    66
231 SSD_Life_Left           PO--C-   100   100   000    -    99
241 Lifetime_Writes_GiB     -O--C-   100   100   000    -    676
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 14
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 14 [13] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 c8 00 00 02 14 c7 e0 40 00  Error: ICRC, ABRT 200 sectors at LBA = 0x0214c7e0 = 34916320

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 c8 00 00 02 14 c7 e0 40 00     00:03:37.477  READ DMA EXT
  25 00 00 01 08 00 00 03 15 4d 00 40 00     00:03:37.476  READ DMA EXT
  25 00 00 01 08 00 00 03 15 4d 18 40 00     00:03:37.475  READ DMA EXT
  25 00 00 01 08 00 00 02 4d 2f d8 40 00     00:03:37.474  READ DMA EXT
  25 00 00 01 08 00 00 03 15 4d 28 40 00     00:03:37.473  READ DMA EXT

Error 13 [12] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 01 08 00 00 02 94 af 20 40 00  Error: ICRC, ABRT 264 sectors at LBA = 0x0294af20 = 43298592

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 08 00 00 02 94 af 20 40 00     00:03:37.450  READ DMA EXT
  25 00 00 01 08 00 00 02 14 c8 a8 40 00     00:03:37.437  READ DMA EXT
  25 00 00 01 13 00 00 02 8d 8a 56 40 00     00:03:37.390  READ DMA EXT
  ff 00 d5 00 01 00 00 00 00 00 01 00 ff     00:03:37.388  [VENDOR SPECIFIC]
  25 00 00 01 13 00 00 02 8d 8a 56 40 00     00:03:37.375  READ DMA EXT

Error 12 [11] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 01 13 00 00 02 8d 8a 56 40 00  Error: ICRC, ABRT 275 sectors at LBA = 0x028d8a56 = 42830422

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 13 00 00 02 8d 8a 56 40 00     00:03:37.375  READ DMA EXT
  25 00 00 00 a9 00 00 02 8d 89 ad 40 00     00:03:37.374  READ DMA EXT
  25 00 00 01 14 00 00 02 8d 88 99 40 00     00:03:37.374  READ DMA EXT
  25 00 00 00 c5 00 00 02 8d 87 d4 40 00     00:03:37.373  READ DMA EXT
  25 00 00 01 08 00 00 02 8d 86 cc 40 00     00:03:37.372  READ DMA EXT

Error 11 [10] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 01 03 00 00 02 8d 6d 35 40 00  Error: ICRC, ABRT 259 sectors at LBA = 0x028d6d35 = 42822965

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 03 00 00 02 8d 6d 35 40 00     00:03:37.280  READ DMA EXT
  25 00 00 00 d1 00 00 02 8d 6c 64 40 00     00:03:37.279  READ DMA EXT
  25 00 00 00 d9 00 00 02 8d 6b 8b 40 00     00:03:37.278  READ DMA EXT
  25 00 00 00 d6 00 00 02 8d 6a b5 40 00     00:03:37.278  READ DMA EXT
  25 00 00 01 16 00 00 02 8d 69 9f 40 00     00:03:37.277  READ DMA EXT

Error 10 [9] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 a2 00 00 02 8d 3d d7 40 00  Error: ICRC, ABRT 162 sectors at LBA = 0x028d3dd7 = 42810839

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 a2 00 00 02 8d 3d d7 40 00     00:03:37.203  READ DMA EXT
  25 00 00 00 a7 00 00 02 8d 3d 30 40 00     00:03:37.203  READ DMA EXT
  25 00 00 00 aa 00 00 02 8d 3c 86 40 00     00:03:37.202  READ DMA EXT
  25 00 00 00 b0 00 00 02 8d 3b d6 40 00     00:03:37.201  READ DMA EXT
  25 00 00 00 b2 00 00 02 8d 3b 24 40 00     00:03:37.201  READ DMA EXT

Error 9 [8] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 b0 00 00 02 8d 35 d4 40 00  Error: ICRC, ABRT 176 sectors at LBA = 0x028d35d4 = 42808788

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 b0 00 00 02 8d 35 d4 40 00     00:03:37.167  READ DMA EXT
  25 00 00 00 a2 00 00 02 8d 35 32 40 00     00:03:37.166  READ DMA EXT
  25 00 00 00 b0 00 00 02 8d 34 82 40 00     00:03:37.165  READ DMA EXT
  25 00 00 00 73 00 00 02 8d 34 0f 40 00     00:03:37.165  READ DMA EXT
  25 00 00 00 b2 00 00 02 8d 33 5d 40 00     00:03:37.164  READ DMA EXT

Error 8 [7] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 01 08 00 00 03 4b bc e8 40 00  Error: ICRC, ABRT 264 sectors at LBA = 0x034bbce8 = 55295208

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 08 00 00 03 4b bc e8 40 00     00:03:27.346  READ DMA EXT
  ff 00 d5 00 01 00 00 00 00 00 01 00 ff     00:03:27.344  [VENDOR SPECIFIC]
  25 00 00 01 08 00 00 03 13 91 60 40 00     00:03:27.331  READ DMA EXT
  25 00 00 01 18 00 00 02 0e 76 30 40 00     00:03:27.330  READ DMA EXT
  25 00 00 01 01 00 00 02 8c d8 80 40 00     00:03:27.316  READ DMA EXT

Error 7 [6] occurred at disk power-on lifetime: 100 hours (4 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 01 01 00 00 00 06 40 28 40 00  Error: ICRC, ABRT 257 sectors at LBA = 0x00064028 = 409640

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 01 00 00 00 06 40 28 40 00     00:03:27.127  READ DMA EXT
  25 00 00 01 10 00 00 00 00 02 28 40 00     00:03:27.116  READ DMA EXT
  25 00 00 01 01 00 00 00 00 00 28 40 00     00:03:27.116  READ DMA EXT
  25 00 00 01 08 00 00 02 46 6a 08 40 00     00:03:27.114  READ DMA EXT
  25 00 00 01 08 00 00 03 15 4d a8 40 00     00:03:27.112  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 1) ==
0x01  0x008  4             236  ---  Lifetime Power-On Resets
0x01  0x010  4             289  ---  Power-on Hours
0x01  0x018  6      1419027194  ---  Logical Sectors Written
0x01  0x028  6       807949326  ---  Logical Sectors Read
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4               0  ---  Number of Reported Uncorrectable Errors
0x05  =====  =               =  ===  == Temperature Statistics (rev 1) ==
0x05  0x008  1              33  ---  Current Temperature
0x05  0x020  1              33  ---  Highest Temperature
0x05  0x028  1              33  ---  Lowest Temperature
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4            1502  ---  Number of Hardware Resets
0x06  0x018  4              66  ---  Number of Interface CRC Errors
0x07  =====  =               =  ===  == Solid State Device Statistics (rev 1) ==
0x07  0x008  1               0  ---  Percentage Used Endurance Indicator
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4           14  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           15  Device-to-host register FISes sent due to a COMRESET
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

