Corsair Solid State Drives
==========================

This is a list of all tested Corsair solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Corsair   | Force 3 SSD        | 240 GB | 2       | 2608  | 0     | 7.15   |
| Corsair   | Force GT           | 240 GB | 1       | 1999  | 0     | 5.48   |
| Corsair   | Force GS           | 128 GB | 2       | 1279  | 0     | 3.51   |
| Corsair   | Force 3 SSD        | 180 GB | 1       | 2914  | 2     | 2.66   |
| Corsair   | Force 3 SSD        | 64 GB  | 4       | 894   | 0     | 2.45   |
| Corsair   | Force LE SSD       | 120 GB | 1       | 811   | 0     | 2.22   |
| Corsair   | Force GT           | 120 GB | 2       | 1377  | 2     | 2.16   |
| Corsair   | Force LS SSD       | 64 GB  | 6       | 1001  | 169   | 1.74   |
| Corsair   | Force GS           | 180 GB | 2       | 631   | 0     | 1.73   |
| Corsair   | CSSD-F60GB2        | 64 GB  | 1       | 516   | 0     | 1.42   |
| Corsair   | Force 3 SSD        | 120 GB | 6       | 934   | 169   | 1.39   |
| Corsair   | CMFSSD-256D1       | 256 GB | 1       | 306   | 0     | 0.84   |
| Corsair   | Force LS SSD       | 120 GB | 3       | 280   | 336   | 0.65   |
| Corsair   | CSSD-V64GB2        | 64 GB  | 1       | 221   | 0     | 0.61   |
| Corsair   | Neutron SSD        | 128 GB | 1       | 202   | 0     | 0.55   |
| Corsair   | FORCE LX SSD       | 256 GB | 1       | 100   | 0     | 0.28   |
| Corsair   | Voyager GTX        | 256 GB | 1       | 13    | 0     | 0.04   |
| Corsair   | Force LX SSD       | 128 GB | 1       | 7     | 0     | 0.02   |
| Corsair   | Force LE SSD       | 240 GB | 1       | 1471  | 285   | 0.01   |
| Corsair   | Neutron GTX SSD    | 120 GB | 1       | 678   | 149   | 0.01   |
| Corsair   | Neutron GTX SSD    | 240 GB | 1       | 374   | 294   | 0.00   |
| Corsair   | CSSD-F80GBP2       | 90 GB  | 1       | 1022  | 1008  | 0.00   |
| Corsair   | Force LS SSD       | 240 GB | 1       | 134   | 1009  | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Corsair   | SandForce Driven SSDs  | 14     | 33      | 1043  | 154   | 2.10   |
| Corsair   | Indilinx Barefoot b... | 2      | 2       | 263   | 0     | 0.72   |
| Corsair   | Unknown                | 6      | 6       | 591   | 122   | 0.47   |
| Corsair   | Silicon Motion base... | 1      | 1       | 100   | 0     | 0.28   |
