smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.9] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.9
Device Model:     ST3808110AS
Serial Number:    --
Firmware Version: 3.AJL
User Capacity:    80,026,361,856 bytes [80.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Sat Jul 10 08:47:19 2021 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (  22)	The self-test routine was aborted by
					the host.
Total time to complete Offline 
data collection: 		(  431) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  27) minutes.
SCT capabilities: 	       (0x0009)	SCT Status supported.
					SCT Error Recovery Control supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000f   100   253   006    Pre-fail  Always       -       0
  3 Spin_Up_Time            0x0002   094   094   000    Old_age   Always       -       0
  4 Start_Stop_Count        0x0033   100   100   020    Pre-fail  Always       -       42
  5 Reallocated_Sector_Ct   0x0033   100   100   036    Pre-fail  Always       -       0
  7 Seek_Error_Rate         0x000f   086   060   030    Pre-fail  Always       -       452799303
  9 Power_On_Hours          0x0032   023   023   000    Old_age   Always       -       68268
 10 Spin_Retry_Count        0x0013   100   100   097    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0033   100   100   020    Pre-fail  Always       -       57
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
189 High_Fly_Writes         0x003a   100   100   000    Old_age   Always       -       0
190 Airflow_Temperature_Cel 0x0022   080   052   045    Old_age   Always       -       20 (Min/Max 17/33)
194 Temperature_Celsius     0x0022   020   048   000    Old_age   Always       -       20 (0 13 0 0 0)
195 Hardware_ECC_Recovered  0x001a   054   045   000    Old_age   Always       -       164711919
197 Current_Pending_Sector  0x0012   100   100   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0010   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x003e   200   200   000    Old_age   Always       -       0
200 Multi_Zone_Error_Rate   0x0000   100   253   000    Old_age   Offline      -       0
202 Data_Address_Mark_Errs  0x0032   100   253   000    Old_age   Always       -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Aborted by host               60%     35864         -
# 2  Short offline       Completed without error       00%     35864         -
# 3  Short offline       Completed without error       00%     35864         -
# 4  Short offline       Completed without error       00%     35864         -
# 5  Short offline       Completed without error       00%     35864         -
# 6  Short offline       Completed without error       00%     35864         -
# 7  Short offline       Completed without error       00%     35864         -
# 8  Short offline       Completed without error       00%     35864         -
# 9  Short offline       Completed without error       00%     35864         -
#10  Short offline       Completed without error       00%     35864         -
#11  Short offline       Completed without error       00%     35863         -
#12  Short offline       Completed without error       00%     35863         -
#13  Short offline       Completed without error       00%     35863         -
#14  Short offline       Completed without error       00%     35863         -
#15  Short offline       Completed without error       00%     35863         -
#16  Short offline       Completed without error       00%     35863         -
#17  Short offline       Completed without error       00%     35863         -
#18  Short offline       Completed without error       00%     35863         -
#19  Short offline       Completed without error       00%     35863         -
#20  Short offline       Completed without error       00%     35863         -
#21  Short offline       Aborted by host               60%     35864         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



