smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.7] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SAMSUNG MZ7PC128HAFU-000L1
Serial Number:    --
Firmware Version: CXM06L1Q
User Capacity:    128,035,676,160 bytes [128 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA8-ACS T13/1699-D revision 4c
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun May 31 12:16:23 2020 AEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  540) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   9) minutes.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  9 Power_On_Hours          0x0032   096   096   000    Old_age   Always       -       16411
 12 Power_Cycle_Count       0x0032   095   095   000    Old_age   Always       -       4790
175 Program_Fail_Count_Chip 0x0032   100   100   010    Old_age   Always       -       0
176 Erase_Fail_Count_Chip   0x0032   100   100   010    Old_age   Always       -       0
177 Wear_Leveling_Count     0x0013   087   087   017    Pre-fail  Always       -       466
178 Used_Rsvd_Blk_Cnt_Chip  0x0013   095   095   010    Pre-fail  Always       -       96
179 Used_Rsvd_Blk_Cnt_Tot   0x0013   095   095   010    Pre-fail  Always       -       176
180 Unused_Rsvd_Blk_Cnt_Tot 0x0013   095   095   010    Pre-fail  Always       -       3856
181 Program_Fail_Cnt_Total  0x0032   100   100   010    Old_age   Always       -       0
182 Erase_Fail_Count_Total  0x0032   100   100   010    Old_age   Always       -       0
183 Runtime_Bad_Block       0x0013   100   100   010    Pre-fail  Always       -       0
184 End-to-End_Error        0x0033   100   100   097    Pre-fail  Always       -       0
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
190 Airflow_Temperature_Cel 0x0032   067   036   000    Old_age   Always       -       33
195 Hardware_ECC_Recovered  0x001a   200   200   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x003e   253   253   000    Old_age   Always       -       0
233 Media_Wearout_Indicator 0x003a   200   200   000    Old_age   Always       -       0
234 Unknown_Attribute       0x0012   100   100   000    Old_age   Always       -       0
235 Unknown_Attribute       0x0012   099   099   000    Old_age   Always       -       41
236 Unknown_Attribute       0x0012   099   099   000    Old_age   Always       -       273
237 Unknown_Attribute       0x0012   099   099   000    Old_age   Always       -       466
238 Unknown_Attribute       0x0012   099   099   000    Old_age   Always       -       176

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

