smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE-p1 amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SanDisk SSD SATA 5000 2.5
Serial Number:    --
Firmware Version: 1.13
User Capacity:    15,804,137,472 bytes [15.8 GB]
Sector Size:      512 bytes logical/physical
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 4a
Local Time is:    Thu Oct 29 10:09:13 2020 MDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (  32)	The self-test routine was interrupted
					by the host with a hard or soft reset.
Total time to complete Offline 
data collection: 		(   60) seconds.
Offline data collection
capabilities: 			 (0x13) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   2) minutes.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   100   100   016    -    0
  2 Throughput_Performance  ------   100   100   040    -    0
  3 Spin_Up_Time            ------   100   100   000    -    0
  4 Start_Stop_Count        ------   100   100   000    -    0
  5 Reallocated_Sector_Ct   ------   100   100   005    -    0
  7 Seek_Error_Rate         ------   100   100   067    -    0
  8 Seek_Time_Performance   ------   100   100   000    -    0
  9 Power_On_Hours          ------   100   100   000    -    0
 10 Spin_Retry_Count        ------   100   100   000    -    0
 11 Calibration_Retry_Count ------   100   100   010    -    0
 12 Power_Cycle_Count       ------   100   100   000    -    0
 13 Read_Soft_Error_Rate    ------   100   100   000    -    0
191 G-Sense_Error_Rate      ------   100   100   000    -    0
192 Power-Off_Retract_Count ------   100   100   000    -    0
194 Temperature_Celsius     ------   100   100   000    -    0
195 Hardware_ECC_Recovered  ------   100   100   000    -    0
196 Reallocated_Event_Count ------   100   100   000    -    0
197 Current_Pending_Sector  ------   100   100   000    -    0
198 Offline_Uncorrectable   ------   100   100   000    -    0
199 UDMA_CRC_Error_Count    ------   100   100   000    -    0
200 Multi_Zone_Error_Rate   ------   100   100   000    -    0
201 Soft_Read_Error_Rate    ------   100   100   000    -    0
223 Load_Retry_Count        ------   100   100   000    -    0
225 Load_Cycle_Count        ------   100   100   000    -    0
232 Available_Reservd_Space ------   073   073   004    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: scsi error aborted command

General Purpose Log Directory Version 0
Address    Access  R/W   Size  Description
0x00       GPL     R/O      1  Log Directory
0x9a       GPL     R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 0
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



