Maxtor Hard Drives
==================

This is a list of all tested Maxtor hard drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ HDD by Model  ](#hdd-by-model)
2. [ HDD by Family ](#hdd-by-family)

HDD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Maxtor    | 6V080E0            | 82 GB  | 1       | 2371  | 0     | 6.50   |
| Maxtor    | STM3250820A        | 250 GB | 1       | 1802  | 0     | 4.94   |
| Maxtor    | 6L080J4            | 80 GB  | 3       | 2093  | 2     | 4.15   |
| Maxtor    | STM3250310AS       | 250 GB | 4       | 927   | 1     | 2.34   |
| Maxtor    | 6V160E0            | 160 GB | 1       | 704   | 0     | 1.93   |
| Maxtor    | 6E040T0            | 40 GB  | 1       | 482   | 0     | 1.32   |
| Maxtor    | STM3160815AS       | 160 GB | 2       | 706   | 480   | 1.11   |
| Maxtor    | STM3250820AS       | 250 GB | 1       | 444   | 5     | 0.20   |
| Maxtor    | STM3320613AS       | 320 GB | 1       | 1639  | 61    | 0.07   |
| Maxtor    | 6L160M0            | 163 GB | 1       | 21    | 0     | 0.06   |
| Maxtor    | 6Y080M0            | 82 GB  | 1       | 31    | 4     | 0.02   |
| Maxtor    | STM380815AS        | 80 GB  | 1       | 2248  | 1008  | 0.01   |
| Maxtor    | 6E030L0            | 32 GB  | 1       | 22    | 10    | 0.01   |
| Maxtor    | 6Y080P0            | 82 GB  | 3       | 15    | 413   | 0.01   |
| Maxtor    | 6Y160M0            | 160 GB | 1       | 7     | 149   | 0.00   |
| Maxtor    | 6E040L0            | 41 GB  | 1       | 20    | 1133  | 0.00   |

HDD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Maxtor    | DiamondMax 10 (SATA... | 2      | 2       | 1537  | 0     | 4.21   |
| Maxtor    | DiamondMax Plus D740X  | 1      | 3       | 2093  | 2     | 4.15   |
| Maxtor    | DiamondMax 21          | 5      | 9       | 1068  | 220   | 1.86   |
| Maxtor    | DiamondMax 8s          | 1      | 1       | 482   | 0     | 1.32   |
| Maxtor    | DiamondMax 22          | 1      | 1       | 1639  | 61    | 0.07   |
| Maxtor    | DiamondMax 10 (ATA/... | 1      | 1       | 21    | 0     | 0.06   |
| Maxtor    | DiamondMax Plus 9      | 3      | 5       | 17    | 279   | 0.01   |
| Maxtor    | DiamondMax Plus 8      | 2      | 2       | 21    | 572   | 0.00   |
