smartctl 7.4 2023-08-01 r5530 [OpenBSD 7.5 amd64] (local build)
Copyright (C) 2002-23, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     INTEL SSDSC2KF180H6L
Serial Number:    --
LU WWN Device Id: 5 5cd2e4 ...
Firmware Version: LSFL37P
User Capacity:    180,045,766,656 bytes [180 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic
Device is:        Not in smartctl database 7.3/5528
ATA Version is:   ACS-3 (minor revision not indicated)
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Wed May 22 16:03:40 2024 BST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x05)	Offline data collection activity
					was aborted by an interrupting command from host.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      ( 246)	Self-test routine in progress...
					60% of test remaining.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x53) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  15) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 1
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  5 Reallocated_Sector_Ct   0x0032   100   100   000    Old_age   Always       -       4
  9 Power_On_Hours          0x0032   100   100   000    Old_age   Always       -       1566
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       1343
170 Unknown_Attribute       0x0033   100   100   010    Pre-fail  Always       -       4
171 Unknown_Attribute       0x0032   100   100   010    Old_age   Always       -       0
172 Unknown_Attribute       0x0032   100   100   010    Old_age   Always       -       0
173 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       65
174 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       221
183 Runtime_Bad_Block       0x0032   100   100   000    Old_age   Always       -       0
184 End-to-End_Error        0x0033   100   100   097    Pre-fail  Always       -       0
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
190 Airflow_Temperature_Cel 0x0032   045   059   000    Old_age   Always       -       45 (Min/Max 22/59)
192 Power-Off_Retract_Count 0x0032   100   100   000    Old_age   Always       -       221
194 Temperature_Celsius     0x0032   045   059   000    Old_age   Always       -       45 (Min/Max 22/59)
199 UDMA_CRC_Error_Count    0x0032   100   100   000    Old_age   Always       -       0
225 Unknown_SSD_Attribute   0x0032   100   100   000    Old_age   Always       -       13467
226 Unknown_SSD_Attribute   0x0032   100   100   000    Old_age   Always       -       0
227 Unknown_SSD_Attribute   0x0032   100   100   000    Old_age   Always       -       0
228 Power-off_Retract_Count 0x0032   100   100   000    Old_age   Always       -       0
232 Available_Reservd_Space 0x0033   099   099   010    Pre-fail  Always       -       0
233 Media_Wearout_Indicator 0x0033   094   094   001    Pre-fail  Always       -       0
236 Unknown_Attribute       0x0033   099   099   001    Pre-fail  Always       -       0
241 Total_LBAs_Written      0x0032   100   100   000    Old_age   Always       -       13467
242 Total_LBAs_Read         0x0032   100   100   000    Old_age   Always       -       21301
249 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       9618

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Extended offline    Self-test routine in progress 60%      1566         -
# 2  Extended offline    Self-test routine in progress 60%      1566         -
# 3  Extended offline    Self-test routine in progress 60%      1566         -
# 4  Extended offline    Self-test routine in progress 60%      1566         -
# 5  Extended offline    Self-test routine in progress 60%      1566         -
# 6  Extended offline    Self-test routine in progress 60%      1566         -
# 7  Extended offline    Self-test routine in progress 60%      1566         -
# 8  Extended offline    Self-test routine in progress 60%      1566         -
# 9  Extended offline    Completed without error       00%      1566         -
#10  Extended offline    Self-test routine in progress 90%      1563         -
#11  Extended offline    Self-test routine in progress 90%      1563         -
#12  Extended offline    Self-test routine in progress 90%      1563         -
#13  Extended offline    Self-test routine in progress 90%      1563         -
#14  Extended offline    Self-test routine in progress 90%      1563         -
#15  Extended offline    Self-test routine in progress 90%      1563         -
#16  Extended offline    Self-test routine in progress 90%      1563         -
#17  Extended offline    Self-test routine in progress 90%      1563         -
#18  Extended offline    Self-test routine in progress 90%      1563         -
#19  Extended offline    Self-test routine in progress 90%      1563         -
#20  Extended offline    Self-test routine in progress 90%      1563         -
#21  Extended offline    Self-test routine in progress 90%      1563         -

SMART Selective self-test log data structure revision number 1
 SPAN         MIN_LBA         MAX_LBA  CURRENT_TEST_STATUS
    1  70403103932424  70403103932424  Not_testing
    2  70403103932424  70403103932424  Not_testing
    3  70403103932424  70403103932424  Not_testing
    4  70403103932424  70403103932424  Not_testing
    5  70403103932424  70403103932424  Not_testing
Selective self-test flags (0x4008):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

The above only provides legacy SMART information - try 'smartctl -x' for more



