smartctl 7.2 2020-12-30 r5155 [OpenBSD 7.0 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Intel 53x and Pro 1500/2500 Series SSDs
Device Model:     INTEL SSDSC2BW240A4
Serial Number:    --
LU WWN Device Id: 5 5cd2e4 ...
Firmware Version: DC32
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available, deterministic
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Thu Jan 20 19:24:46 2022 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x05)	Offline data collection activity
					was aborted by an interrupting command from host.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (  33)	The self-test routine was interrupted
					by the host with a hard or soft reset.
Total time to complete Offline 
data collection: 		( 5860) seconds.
Offline data collection
capabilities: 			 (0x7f) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Abort Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  48) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x0025)	SCT Status supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  5 Reallocated_Sector_Ct   0x0032   100   100   000    Old_age   Always       -       0
  9 Power_On_Hours_and_Msec 0x0032   100   100   000    Old_age   Always       -       19391h+40m+22.040s
 12 Power_Cycle_Count       0x0032   099   099   000    Old_age   Always       -       1657
170 Available_Reservd_Space 0x0033   100   100   010    Pre-fail  Always       -       0
171 Program_Fail_Count      0x0032   100   100   000    Old_age   Always       -       0
172 Erase_Fail_Count        0x0032   100   100   000    Old_age   Always       -       0
174 Unexpect_Power_Loss_Ct  0x0032   100   100   000    Old_age   Always       -       70
183 SATA_Downshift_Count    0x0032   100   100   000    Old_age   Always       -       208
184 End-to-End_Error        0x0033   100   100   090    Pre-fail  Always       -       0
187 Uncorrectable_Error_Cnt 0x0032   100   100   000    Old_age   Always       -       0
190 Airflow_Temperature_Cel 0x0032   029   054   000    Old_age   Always       -       29 (Min/Max 19/54)
192 Power-Off_Retract_Count 0x0032   100   100   000    Old_age   Always       -       70
199 UDMA_CRC_Error_Count    0x0032   100   100   000    Old_age   Always       -       0
225 Host_Writes_32MiB       0x0032   100   100   000    Old_age   Always       -       1412336
226 Workld_Media_Wear_Indic 0x0032   100   100   000    Old_age   Always       -       65535
227 Workld_Host_Reads_Perc  0x0032   100   100   000    Old_age   Always       -       38
228 Workload_Minutes        0x0032   100   100   000    Old_age   Always       -       65535
232 Available_Reservd_Space 0x0033   100   100   010    Pre-fail  Always       -       0
233 Media_Wearout_Indicator 0x0032   074   074   000    Old_age   Always       -       0
241 Host_Writes_32MiB       0x0032   100   100   000    Old_age   Always       -       1412336
242 Host_Reads_32MiB        0x0032   100   100   000    Old_age   Always       -       874957
249 NAND_Writes_1GiB        0x0032   100   100   000    Old_age   Always       -       182870

SMART Error Log not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Offline             Interrupted (host reset)      10%     19390         -
# 2  Offline             Interrupted (host reset)      10%     19387         -
# 3  Offline             Interrupted (host reset)      10%     19384         -
# 4  Offline             Interrupted (host reset)      10%     19382         -
# 5  Offline             Interrupted (host reset)      10%     19382         -
# 6  Offline             Interrupted (host reset)      10%     19373         -
# 7  Offline             Interrupted (host reset)      10%     19358         -
# 8  Offline             Interrupted (host reset)      10%     19358         -
# 9  Offline             Interrupted (host reset)      10%     19357         -
#10  Offline             Interrupted (host reset)      10%     19351         -
#11  Offline             Interrupted (host reset)      10%     19345         -
#12  Offline             Interrupted (host reset)      10%     19339         -
#13  Offline             Interrupted (host reset)      10%     19333         -
#14  Offline             Interrupted (host reset)      10%     19327         -
#15  Offline             Interrupted (host reset)      10%     19313         -
#16  Offline             Interrupted (host reset)      10%     19298         -
#17  Offline             Interrupted (host reset)      10%     19290         -
#18  Offline             Interrupted (host reset)      10%     19279         -
#19  Offline             Interrupted (host reset)      10%     19276         -
#20  Offline             Interrupted (host reset)      10%     19269         -
#21  Offline             Interrupted (host reset)      10%     19263         -

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



