smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.8] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Intel X25-E SSDs
Device Model:     SSDSA2SH064G1GC INTEL
Serial Number:    --
LU WWN Device Id: 5 001517 ...
Firmware Version: 045C8860
User Capacity:    64,023,257,088 bytes [64.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 1
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Sun Dec  6 04:24:59 2020 PST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (  32)	The self-test routine was interrupted
					by the host with a hard or soft reset.
Total time to complete Offline 
data collection: 		(    1) seconds.
Offline data collection
capabilities: 			 (0x75) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Abort Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   4) minutes.
Conveyance self-test routine
recommended polling time: 	 (   1) minutes.

SMART Attributes Data Structure revision number: 5
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  3 Spin_Up_Time            0x0000   100   000   000    Old_age   Offline      -       0
  4 Start_Stop_Count        0x0000   100   000   000    Old_age   Offline      -       0
  5 Reallocated_Sector_Ct   0x0002   100   100   000    Old_age   Always       -       0
  9 Power_On_Hours          0x0002   100   100   000    Old_age   Always       -       4309
 12 Power_Cycle_Count       0x0002   100   100   000    Old_age   Always       -       1804
192 Unsafe_Shutdown_Count   0x0002   100   100   000    Old_age   Always       -       1030
232 Available_Reservd_Space 0x0003   100   100   010    Pre-fail  Always       -       0
233 Media_Wearout_Indicator 0x0002   099   099   000    Old_age   Always       -       0
225 Host_Writes_32MiB       0x0000   200   200   000    Old_age   Offline      -       91067
226 Intel_Internal          0x0002   255   000   000    Old_age   Always       -       0
227 Intel_Internal          0x0002   000   000   000    Old_age   Always       -       0
228 Intel_Internal          0x0002   000   000   000    Old_age   Always       -       0

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%       318         -
# 2  Short offline       Completed without error       00%       198         -
# 3  Short offline       Completed without error       00%       181         -
# 4  Short offline       Completed without error       00%       179         -
# 5  Short offline       Completed without error       00%       179         -
# 6  Short offline       Completed without error       00%       179         -
# 7  Short offline       Completed without error       00%       176         -
# 8  Short offline       Completed without error       00%       176         -
# 9  Short offline       Completed without error       00%       175         -
#10  Short offline       Completed without error       00%       172         -
#11  Short offline       Completed without error       00%       169         -
#12  Short offline       Completed without error       00%       146         -
#13  Short offline       Completed without error       00%       123         -
#14  Short offline       Completed without error       00%       104         -
#15  Short offline       Completed without error       00%       102         -
#16  Short offline       Completed without error       00%       102         -
#17  Short offline       Completed without error       00%        91         -

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

