Samsung Hard Drives
===================

This is a list of all tested Samsung hard drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ HDD by Model  ](#hdd-by-model)
2. [ HDD by Family ](#hdd-by-family)

HDD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Samsung   | HD502IJ            | 500 GB | 2       | 2696  | 1     | 6.93   |
| Samsung   | HD204UI            | 2 TB   | 20      | 2071  | 7     | 4.30   |
| Samsung   | HD502HI            | 500 GB | 2       | 1402  | 0     | 3.84   |
| Samsung   | HD322HJ            | 320 GB | 10      | 1548  | 61    | 3.69   |
| Samsung   | HD154UI            | 1.5 TB | 8       | 2606  | 276   | 3.52   |
| Samsung   | HD161GJ            | 160 GB | 3       | 1263  | 0     | 3.46   |
| Samsung   | HD103SJ            | 1 TB   | 9       | 1786  | 227   | 3.38   |
| Samsung   | HD251HJ            | 250 GB | 2       | 1071  | 0     | 2.94   |
| Samsung   | HD502HJ            | 500 GB | 9       | 1589  | 1     | 2.86   |
| Samsung   | HD103UJ            | 1 TB   | 9       | 1787  | 27    | 2.79   |
| Samsung   | HM500JI            | 500 GB | 4       | 1251  | 53    | 2.71   |
| Samsung   | HD501LJ            | 500 GB | 12      | 2110  | 256   | 2.64   |
| Samsung   | HD753LJ            | 752 GB | 4       | 1723  | 423   | 2.40   |
| Samsung   | HD103SI            | 1 TB   | 5       | 823   | 606   | 1.91   |
| Samsung   | HM250HI            | 250 GB | 6       | 626   | 14    | 1.58   |
| Samsung   | HD250HJ            | 250 GB | 2       | 1028  | 1211  | 1.49   |
| Samsung   | HD161HJ            | 160 GB | 7       | 755   | 377   | 1.27   |
| Samsung   | HM321HI            | 320 GB | 6       | 373   | 145   | 0.94   |
| Samsung   | HM320II            | 320 GB | 5       | 628   | 1     | 0.78   |
| Samsung   | HN-M101MBB         | 1 TB   | 2       | 255   | 0     | 0.70   |
| Samsung   | HM250JI            | 250 GB | 2       | 309   | 506   | 0.41   |
| Samsung   | HM160HI            | 160 GB | 9       | 424   | 150   | 0.12   |
| Samsung   | HM251JI            | 250 GB | 2       | 75    | 14    | 0.10   |
| Samsung   | HM320JI            | 320 GB | 4       | 351   | 137   | 0.05   |
| Samsung   | SP2004C            | 200 GB | 2       | 747   | 509   | 0.04   |
| Samsung   | HD321KJ            | 320 GB | 2       | 1606  | 1016  | 0.00   |
| Samsung   | HD642JJ            | 640 GB | 2       | 1044  | 1351  | 0.00   |

HDD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Samsung   | SpinPoint F4 EG (AF)   | 1      | 20      | 2071  | 7     | 4.30   |
| Samsung   | SpinPoint F1 DT        | 7      | 32      | 1621  | 164   | 3.18   |
| Samsung   | SpinPoint F3           | 2      | 18      | 1687  | 114   | 3.12   |
| Samsung   | SpinPoint F2 EG        | 3      | 15      | 1851  | 349   | 3.02   |
| Samsung   | SpinPoint T166         | 2      | 14      | 2038  | 365   | 2.26   |
| Samsung   | SpinPoint M7           | 3      | 15      | 793   | 20    | 1.61   |
| Samsung   | SpinPoint S250         | 1      | 2       | 1028  | 1211  | 1.49   |
| Samsung   | SpinPoint S166         | 1      | 7       | 755   | 377   | 1.27   |
| Samsung   | SpinPoint M7E (AF)     | 1      | 6       | 373   | 145   | 0.94   |
| Samsung   | SpinPoint M8 (AF)      | 1      | 2       | 255   | 0     | 0.70   |
| Samsung   | SpinPoint M5           | 2      | 11      | 403   | 215   | 0.18   |
| Samsung   | SpinPoint M6           | 2      | 6       | 259   | 96    | 0.07   |
| Samsung   | SpinPoint P120         | 1      | 2       | 747   | 509   | 0.04   |
