smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p6 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     DEM24-64GM41BC1DC-PC
Serial Number:    --
LU WWN Device Id: 5 02b2a2 ...
Firmware Version: L19620
User Capacity:    64,023,257,088 bytes [64.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available, deterministic, zeroed
Device is:        Not in smartctl database 7.3/5319
ATA Version is:   ACS-3 T13/2161-D revision 4
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Mon Feb 20 19:26:25 2023 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(   32) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					General Purpose Logging supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
  2 Throughput_Performance  ------   000   000   000    -    0
  3 Spin_Up_Time            ------   000   000   000    -    0
  5 Reallocated_Sector_Ct   -O--C-   100   100   001    -    0
  7 Unknown_SSD_Attribute   ------   000   000   000    -    0
  8 Unknown_SSD_Attribute   ------   000   000   000    -    0
  9 Power_On_Hours          -O--C-   123   000   000    -    1741
 10 Unknown_SSD_Attribute   ------   000   000   000    -    0
 12 Power_Cycle_Count       -O--C-   232   000   000    -    232
163 Unknown_Attribute       ------   000   000   000    -    7
168 Unknown_Attribute       ------   000   000   000    -    0
169 Unknown_Attribute       ------   100   000   000    -    100
175 Program_Fail_Count_Chip ------   000   000   000    -    0
192 Power-Off_Retract_Count -O--C-   000   000   000    -    63
194 Temperature_Celsius     -O----   046   100   000    -    46 (3 51 0 38 0)
197 Current_Pending_Sector  ------   000   000   000    -    0
225 Unknown_SSD_Attribute   ------   000   000   000    -    0
240 Unknown_SSD_Attribute   ------   000   000   000    -    0
165 Unknown_Attribute       -O--C-   030   100   000    -    30
167 Unknown_Attribute       -O--C-   000   100   000    -    9
170 Unknown_Attribute       PO--C-   100   100   010    -    144
171 Unknown_Attribute       -O--C-   000   100   000    -    0
172 Unknown_Attribute       -O--C-   000   100   000    -    0
176 Erase_Fail_Count_Chip   ------   000   000   000    -    0
187 Reported_Uncorrect      -O--C-   000   000   000    -    0
229 Unknown_Attribute       ------   100   100   000    -    89569723955864
232 Available_Reservd_Space PO--C-   000   000   000    -    0
235 Unknown_Attribute       -O----   000   000   000    -    0
241 Total_LBAs_Written      -O----   100   100   000    -    12165
242 Total_LBAs_Read         -O----   100   100   000    -    13261
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xdf       GPL,SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log not supported

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       20%         0         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported

