Micron NVMe Drives
==================

This is a list of all tested Micron NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Micron    | 7300_MTFDHBA400TDG | 400 GB | 2       | 272   | 0     | 0.75   |
| Micron    | 2200S NVMe         | 256 GB | 3       | 198   | 0     | 0.54   |
| Micron    | MTFDHBA256TCK-1... | 256 GB | 2       | 193   | 0     | 0.53   |
| Micron    | 2300_MTFDHBA512TDV | 512 GB | 2       | 113   | 0     | 0.31   |
| Micron    | 2200S NVMe         | 1 TB   | 3       | 92    | 0     | 0.25   |
| Micron    | 2210_MTFDHBA512QFD | 512 GB | 2       | 71    | 0     | 0.19   |
| Micron    | 2200V_MTFDHBA51... | 512 GB | 3       | 54    | 0     | 0.15   |
| Micron    | 2200S NVMe         | 512 GB | 3       | 43    | 0     | 0.12   |
| Micron    | MTFDHBA512QFD-1... | 512 GB | 2       | 37    | 0     | 0.10   |
| Micron    | 2300 NVMe          | 512 GB | 3       | 21    | 0     | 0.06   |
| Micron    | 7450_MTFDKBA800TFS |        | 2       | 19    | 0     | 0.05   |
| Micron    | 2450_MTFDKBA1T0TFK | 1 TB   | 2       | 17    | 0     | 0.05   |
