Intel NVMe Drives
=================

This is a list of all tested Intel NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Intel     | SSDPEDMW400G4      | 400 GB | 2       | 1410  | 0     | 3.86   |
| Intel     | SSDPE2MX450G7      | 450 GB | 2       | 1077  | 0     | 2.95   |
| Intel     | SSDPED1D280GA      | 280 GB | 2       | 1036  | 0     | 2.84   |
| Intel     | SSDPEDKX040T7      | 4 TB   | 2       | 998   | 0     | 2.74   |
| Intel     | SSDPE21D280GA      | 280 GB | 2       | 543   | 0     | 1.49   |
| Intel     | SSDPEKKW128G8      | 128 GB | 2       | 494   | 0     | 1.35   |
| Intel     | SSDPEKKW256G8      | 256 GB | 3       | 490   | 0     | 1.34   |
| Intel     | MEMPEK1W016GA      | 16 GB  | 3       | 439   | 0     | 1.20   |
| Intel     | SSDPEKKW128G7      | 128 GB | 2       | 840   | 1     | 1.15   |
| Intel     | SSDPEKNW512G8      | 512 GB | 11      | 262   | 0     | 0.72   |
| Intel     | SSDPEKNW020T8      | 2 TB   | 7       | 239   | 0     | 0.66   |
| Intel     | SSDPEKNW010T8      | 1 TB   | 6       | 192   | 0     | 0.53   |
| Intel     | HBRPEKNX0101AH     | 256 GB | 2       | 192   | 0     | 0.53   |
| Intel     | SSDPEKKF256G8L     | 256 GB | 9       | 166   | 0     | 0.46   |
| Intel     | SSDPEKNW512G8H     | 512 GB | 7       | 164   | 0     | 0.45   |
| Intel     | HBRPEKNX0202AH     | 512 GB | 2       | 154   | 0     | 0.42   |
| Intel     | HBRPEKNX0202AHO    | 32 GB  | 2       | 154   | 0     | 0.42   |
| Intel     | MEMPEK1J016GAH     | 16 GB  | 3       | 152   | 0     | 0.42   |
| Intel     | SSDPEKKF512G8L     | 512 GB | 7       | 145   | 0     | 0.40   |
| Intel     | HBRPEKNX0203AH     | 1 TB   | 2       | 127   | 0     | 0.35   |
| Intel     | SSDPEKKW512G7      | 512 GB | 2       | 174   | 1     | 0.30   |
| Intel     | MEMPEK1W032GA      | 32 GB  | 5       | 69    | 0     | 0.19   |
| Intel     | SSDPEKNW010T9      | 1 TB   | 2       | 27    | 0     | 0.07   |
| Intel     | SSDPEKNU512GZ      | 512 GB | 4       | 11    | 0     | 0.03   |
