Crucial NVMe Drives
===================

This is a list of all tested Crucial NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Crucial   | CT500P1SSD8        | 500 GB | 8       | 289   | 0     | 0.79   |
| Crucial   | CT500P5PSSD8       | 500 GB | 2       | 199   | 0     | 0.55   |
| Crucial   | CT1000P1SSD8       | 1 TB   | 13      | 184   | 15    | 0.47   |
| Crucial   | CT1000P2SSD8       | 1 TB   | 10      | 143   | 0     | 0.39   |
| Crucial   | CT2000P2SSD8       | 2 TB   | 3       | 97    | 0     | 0.27   |
| Crucial   | CT500P2SSD8        | 500 GB | 13      | 73    | 0     | 0.20   |
| Crucial   | CT250P2SSD8        | 250 GB | 15      | 66    | 0     | 0.18   |
| Crucial   | CT500P5SSD8        | 500 GB | 4       | 57    | 0     | 0.16   |
| Crucial   | CT1000P5SSD8       | 1 TB   | 7       | 32    | 0     | 0.09   |
| Crucial   | CT500P3SSD8        | 500 GB | 5       | 21    | 0     | 0.06   |
| Crucial   | CT2000P3SSD8       | 2 TB   | 2       | 11    | 0     | 0.03   |
