Plextor Solid State Drives
==========================

This is a list of all tested Plextor solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Plextor   | PX-512M5Pro        | 512 GB | 1       | 1381  | 0     | 3.79   |
| Plextor   | PH6-CE120          | 120 GB | 1       | 864   | 0     | 2.37   |
| Plextor   | PH6-CE120-G        | 120 GB | 1       | 804   | 0     | 2.20   |
| Plextor   | PX-64G5Le          | 64 GB  | 1       | 793   | 0     | 2.17   |
| Plextor   | PX-128M7VC         | 128 GB | 1       | 671   | 0     | 1.84   |
| Plextor   | PX-AG256M6e        | 256 GB | 1       | 576   | 0     | 1.58   |
| Plextor   | PX-64G7Me          | 64 GB  | 1       | 489   | 0     | 1.34   |
| Plextor   | PX-256M5Pro        | 256 GB | 1       | 392   | 0     | 1.07   |
| Plextor   | PX-512M8VC         | 512 GB | 1       | 300   | 0     | 0.82   |
| Plextor   | PX-128M5S          | 128 GB | 1       | 1216  | 4     | 0.67   |
| Plextor   | PX-256M8VG         | 256 GB | 1       | 230   | 0     | 0.63   |
| Plextor   | PX-128M5Pro        | 128 GB | 1       | 224   | 0     | 0.61   |
| Plextor   | PX-128S3C          | 128 GB | 1       | 213   | 0     | 0.58   |
| Plextor   | PX-256M8VC         | 256 GB | 1       | 184   | 0     | 0.51   |
| Plextor   | PX-64M5M           | 64 GB  | 1       | 154   | 0     | 0.42   |
| Plextor   | PX-256M5M          | 256 GB | 1       | 135   | 0     | 0.37   |
| Plextor   | PX-128M5M          | 128 GB | 3       | 89    | 0     | 0.25   |
| Plextor   | PX-256M5S          | 256 GB | 2       | 64    | 0     | 0.18   |
| Plextor   | PX-128M6S          | 128 GB | 2       | 50    | 0     | 0.14   |
| Plextor   | PX-128G7Ne         | 128 GB | 1       | 189   | 6     | 0.07   |
| Plextor   | PH6-CE240          | 240 GB | 1       | 4     | 0     | 0.01   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Plextor   | Unknown                | 11     | 11      | 422   | 1     | 1.12   |
| Plextor   | M3/M5/M6/M7 Series ... | 9      | 12      | 378   | 1     | 0.82   |
| Plextor   | M3/M5/M6 Series SSDs   | 1      | 2       | 64    | 0     | 0.18   |
