Intel NVMe Drives
=================

This is a list of all tested Intel NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Intel     | SSDPEDMW400G4      | 400 GB | 2       | 1410  | 0     | 3.86   |
| Intel     | SSDPEDME016T4S     | 1.6 TB | 1       | 1203  | 0     | 3.30   |
| Intel     | SSDPE2MX450G7      | 450 GB | 2       | 1077  | 0     | 2.95   |
| Intel     | SSDPED1D280GA      | 280 GB | 2       | 1036  | 0     | 2.84   |
| Intel     | SSDPED1D480GA      | 480 GB | 1       | 979   | 0     | 2.68   |
| Intel     | SSDPEKKF256G7L     | 256 GB | 1       | 827   | 0     | 2.27   |
| Intel     | SSDPE21D280GA      | 280 GB | 2       | 543   | 0     | 1.49   |
| Intel     | SSDPEKNW010T8H     | 1 TB   | 1       | 494   | 0     | 1.36   |
| Intel     | SSDPEKKW128G8      | 128 GB | 2       | 494   | 0     | 1.35   |
| Intel     | SSDPEKKW256G8      | 256 GB | 3       | 490   | 0     | 1.34   |
| Intel     | MEMPEK1W016GA      | 16 GB  | 3       | 439   | 0     | 1.20   |
| Intel     | SSDPEKKW128G7      | 128 GB | 2       | 840   | 1     | 1.15   |
| Intel     | SSDPEKKW512G8      | 512 GB | 1       | 310   | 0     | 0.85   |
| Intel     | SSDPEKNW020T8      | 2 TB   | 7       | 239   | 0     | 0.66   |
| Intel     | SSDPEKNW512G8      | 512 GB | 9       | 237   | 0     | 0.65   |
| Intel     | MEMPEK1J016GAD     | 16 GB  | 1       | 235   | 0     | 0.65   |
| Intel     | SSDPEKNW010T8      | 1 TB   | 5       | 198   | 0     | 0.54   |
| Intel     | HBRPEKNX0101AH     | 256 GB | 2       | 192   | 0     | 0.53   |
| Intel     | SSDPEKKF256G8L     | 256 GB | 6       | 186   | 0     | 0.51   |
| Intel     | SSDPEDMW800G4      | 800 GB | 1       | 168   | 0     | 0.46   |
| Intel     | SSDPEKKF512G8L     | 512 GB | 6       | 159   | 0     | 0.44   |
| Intel     | HBRPEKNX0202AH     | 512 GB | 2       | 154   | 0     | 0.42   |
| Intel     | HBRPEKNX0202AHO    | 32 GB  | 2       | 154   | 0     | 0.42   |
| Intel     | MEMPEK1J016GAH     | 16 GB  | 3       | 152   | 0     | 0.42   |
| Intel     | SSDPEKNW512G8H     | 512 GB | 6       | 137   | 0     | 0.38   |
| Intel     | SSDPEL1K100GA      | 100 GB | 1       | 123   | 0     | 0.34   |
| Intel     | SSDPEKKW512G7      | 512 GB | 2       | 174   | 1     | 0.30   |
| Intel     | SSDPEKKW256G8L     | 256 GB | 1       | 89    | 0     | 0.24   |
| Intel     | MEMPEK1W032GA      | 32 GB  | 5       | 69    | 0     | 0.19   |
| Intel     | HBRPEKNX0203AHO    | 32 GB  | 1       | 55    | 0     | 0.15   |
| Intel     | HBRPEKNX0203AH     | 1 TB   | 1       | 52    | 0     | 0.14   |
| Intel     | SSDPEK1A118GA      | 118 GB | 1       | 26    | 0     | 0.07   |
| Intel     | SSDPEKNW010T9      | 1 TB   | 1       | 25    | 0     | 0.07   |
| Intel     | SSDPEKNU512GZ      | 512 GB | 2       | 8     | 0     | 0.02   |
| Intel     | MEMPEK1J016GAL     | 16 GB  | 1       | 3     | 0     | 0.01   |
| Intel     | 670p SSDPEKNU51... | 512 GB | 1       | 2     | 0     | 0.01   |
| Intel     | SSDPEKKW010T7      | 1 TB   | 1       | 0     | 0     | 0.00   |
