Transcend NVMe Drives
=====================

This is a list of all tested Transcend NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Transcend | TS256GMTE110S      | 256 GB | 1       | 730   | 0     | 2.00   |
| Transcend | TS500GMTE240S      | 500 GB | 2       | 214   | 0     | 0.59   |
| Transcend | TS128GMTE110S      | 128 GB | 12      | 133   | 0     | 0.37   |
| Transcend | TS2TMTE220S        | 2 TB   | 2       | 90    | 0     | 0.25   |
| Transcend | TS256GMTE220S      | 256 GB | 1       | 60    | 0     | 0.17   |
| Transcend | TS256GMTE652T2     | 256 GB | 16      | 11    | 0     | 0.03   |
| Transcend | TS1TMTE110S        | 1 TB   | 1       | 0     | 0     | 0.00   |
