Toshiba Solid State Drives
==========================

This is a list of all tested Toshiba solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Toshiba   | THNSNH256GMCT      | 256 GB | 2       | 2007  | 0     | 5.50   |
| Toshiba   | TR150              | 120 GB | 1       | 1746  | 0     | 4.79   |
| Toshiba   | THNSNH512GBST      | 512 GB | 1       | 1700  | 0     | 4.66   |
| Toshiba   | THNSNX032GTNT M... | 32 GB  | 1       | 1665  | 0     | 4.56   |
| Toshiba   | THNSNJ128GCSY      | 128 GB | 2       | 1388  | 0     | 3.80   |
| Toshiba   | THNSNH128GBST      | 128 GB | 3       | 1234  | 0     | 3.38   |
| Toshiba   | THNSF8120CCSE      | 120 GB | 1       | 1126  | 0     | 3.09   |
| Toshiba   | THNSNH060GCST      | 64 GB  | 1       | 1105  | 0     | 3.03   |
| Toshiba   | THNSNJ128GCSU      | 128 GB | 5       | 1009  | 0     | 2.77   |
| Toshiba   | THNSFJ256GDNU      | 256 GB | 2       | 986   | 0     | 2.70   |
| Toshiba   | THNSNJ128GMCU      | 128 GB | 2       | 911   | 0     | 2.50   |
| Toshiba   | THNSNF128GMCS      | 128 GB | 2       | 831   | 0     | 2.28   |
| Toshiba   | THNSNC128GBSJ      | 128 GB | 1       | 826   | 0     | 2.26   |
| Toshiba   | Q300               | 480 GB | 2       | 762   | 0     | 2.09   |
| Toshiba   | Q300               | 120 GB | 1       | 740   | 0     | 2.03   |
| Toshiba   | TL100              | 240 GB | 1       | 707   | 0     | 1.94   |
| Toshiba   | THNSNC128GMLJ      | 128 GB | 1       | 692   | 0     | 1.90   |
| Toshiba   | THNSNF256GMCS      | 256 GB | 1       | 690   | 0     | 1.89   |
| Toshiba   | THNSFJ256GCSU      | 256 GB | 4       | 553   | 0     | 1.52   |
| Toshiba   | A100               | 240 GB | 1       | 503   | 0     | 1.38   |
| Toshiba   | Q300 Pro           | 128 GB | 2       | 494   | 0     | 1.35   |
| Toshiba   | THNSFJ128GMCT      | 128 GB | 1       | 462   | 0     | 1.27   |
| Toshiba   | THNSNJ128GCST      | 128 GB | 1       | 422   | 0     | 1.16   |
| Toshiba   | THNSNF128GCSS      | 128 GB | 2       | 419   | 0     | 1.15   |
| Toshiba   | TR200              | 240 GB | 8       | 388   | 0     | 1.07   |
| Toshiba   | TR200              | 480 GB | 1       | 358   | 0     | 0.98   |
| Toshiba   | THNSNX032GTNT      | 32 GB  | 1       | 312   | 0     | 0.86   |
| Toshiba   | Q300               | 240 GB | 2       | 209   | 0     | 0.57   |
| Toshiba   | KSG60ZMV256G M.... | 256 GB | 6       | 205   | 17    | 0.48   |
| Toshiba   | THNSNJ256GCSY      | 256 GB | 2       | 175   | 0     | 0.48   |
| Toshiba   | THNSNC064GBSJ      | 64 GB  | 1       | 115   | 0     | 0.32   |
| Toshiba   | TL100              | 120 GB | 1       | 30    | 0     | 0.08   |
| Toshiba   | VT180              | 480 GB | 2       | 20    | 0     | 0.06   |
| Toshiba   | KSG60ZMV256G       | 256 GB | 1       | 12    | 0     | 0.03   |
| Toshiba   | THNSNK256GVN8 M... | 256 GB | 1       | 678   | 100   | 0.02   |
| Toshiba   | KSG60ZSE256G SATA  | 256 GB | 1       | 468   | 100   | 0.01   |
| Toshiba   | THNSNH128GCST      | 128 GB | 1       | 4     | 0     | 0.01   |
| Toshiba   | THNSNK256GCS8 SATA | 256 GB | 1       | 373   | 100   | 0.01   |
| Toshiba   | THNSNK128GCS8 SATA | 128 GB | 2       | 206   | 100   | 0.01   |
| Toshiba   | THNSNK512GVN8      | 512 GB | 1       | 137   | 692   | 0.00   |
| Toshiba   | THNSNX024GMNT      | 24 GB  | 1       | 0     | 2     | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Toshiba   | OCZ/Toshiba Trion SSDs | 1      | 1       | 1746  | 0     | 4.79   |
| Toshiba   | HG5d Series            | 3      | 5       | 963   | 0     | 2.64   |
| Toshiba   | HG5 Series             | 1      | 2       | 831   | 0     | 2.28   |
| Toshiba   | HG3 Series             | 1      | 1       | 826   | 0     | 2.26   |
| Toshiba   | HG6 Series SSD         | 6      | 15      | 796   | 0     | 2.18   |
| Toshiba   | JMicron/Maxiotek ba... | 1      | 1       | 692   | 0     | 1.90   |
| Toshiba   | Unknown                | 25     | 45      | 545   | 29    | 1.36   |
| Toshiba   | OCZ                    | 3      | 4       | 194   | 0     | 0.53   |
