Patriot Solid State Drives
==========================

This is a list of all tested Patriot solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Patriot   | Ignite M3          | 120 GB | 1       | 1831  | 0     | 5.02   |
| Patriot   | Flare              | 64 GB  | 2       | 1107  | 0     | 3.03   |
| Patriot   | Pyro               | 64 GB  | 1       | 1039  | 0     | 2.85   |
| Patriot   | Blaze              | 64 GB  | 2       | 1006  | 0     | 2.76   |
| Patriot   | FLARE              | 64 GB  | 1       | 562   | 0     | 1.54   |
| Patriot   | Burst              | 480 GB | 2       | 455   | 0     | 1.25   |
| Patriot   | Pyro SSD           | 240 GB | 1       | 409   | 0     | 1.12   |
| Patriot   | Burst              | 240 GB | 8       | 391   | 0     | 1.07   |
| Patriot   | Burst              | 960 GB | 2       | 378   | 0     | 1.04   |
| Patriot   | Burst Elite        | 240 GB | 1       | 266   | 0     | 0.73   |
| Patriot   | Burst              | 120 GB | 13      | 203   | 0     | 0.56   |
| Patriot   | Burst Elite        | 120 GB | 5       | 37    | 0     | 0.10   |
| Patriot   | Inferno 60GB SSD   | 64 GB  | 1       | 936   | 96    | 0.03   |
| Patriot   | Burst Elite        | 480 GB | 1       | 0     | 0     | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Patriot   | SandForce Driven SSDs  | 1      | 1       | 1039  | 0     | 2.85   |
| Patriot   | Phison Driven SSDs     | 6      | 29      | 402   | 0     | 1.10   |
| Patriot   | Unknown                | 7      | 11      | 381   | 9     | 0.81   |
