smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       LENSE20256GMSP34MEAT2TA
Serial Number:                      --
Firmware Version:                   2.8.8341
PCI Vendor/Subsystem ID:            0x17aa
IEEE OUI Identifier:                0xa03299
Controller ID:                      1
NVMe Version:                       <1.2
Number of Namespaces:               1
Namespace 1 Size/Capacity:          256,060,514,304 [256 GB]
Namespace 1 Utilization:            0
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            a03299 ...
Local Time is:                      Sun Jan 22 12:05:23 2023 UTC
Firmware Updates (0x02):            1 Slot
Optional Admin Commands (0x0007):   Security Format Frmw_DL
Optional NVM Commands (0x0016):     Wr_Unc DS_Mngmt Sav/Sel_Feat
Maximum Data Transfer Size:         32 Pages
Warning  Comp. Temp. Threshold:     70 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     6.50W       -        -    0  0  0  0        0       0
 1 +     4.60W       -        -    1  1  1  1        5       5
 2 +     3.90W       -        -    2  2  2  2        5       5
 3 -   0.1000W       -        -    3  3  3  3    35000    6000
 4 -   0.0100W       -        -    4  4  4  4    35000    6000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 -     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        40 Celsius
Available Spare:                    100%
Available Spare Threshold:          3%
Percentage Used:                    8%
Data Units Read:                    41,562,287 [21.2 TB]
Data Units Written:                 26,183,343 [13.4 TB]
Host Read Commands:                 1,310,805,208
Host Write Commands:                676,098,604
Controller Busy Time:               5,391
Power Cycles:                       1,532
Power On Hours:                     4,419
Unsafe Shutdowns:                   102
Media and Data Integrity Errors:    0
Error Information Log Entries:      0
Warning  Comp. Temperature Time:    0
Temperature Sensor 1:               53 Celsius
Temperature Sensor 2:               40 Celsius
Temperature Sensor 3:               35 Celsius

Error Information (NVMe Log 0x01, 4 of 4 entries)
No Errors Logged

