HP Solid State Drives
=====================

This is a list of all tested HP solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| HP        | VK0800GDJYA        | 800 GB | 1       | 1986  | 0     | 5.44   |
| HP        | FK0032CAAZP        | 32 GB  | 3       | 1371  | 0     | 3.76   |
| HP        | VK0480GECQP        | 480 GB | 1       | 1083  | 0     | 2.97   |
| HP        | SSD M700           | 240 GB | 1       | 487   | 0     | 1.34   |
| HP        | SSD S700 Pro       | 256 GB | 1       | 400   | 0     | 1.10   |
| HP        | SSD S600           | 120 GB | 1       | 339   | 0     | 0.93   |
| HP        | SSD S700 Pro       | 512 GB | 2       | 294   | 0     | 0.81   |
| HP        | SSD S700           | 250 GB | 5       | 264   | 0     | 0.72   |
| HP        | SSD S700           | 1 TB   | 1       | 198   | 0     | 0.54   |
| HP        | SSD S600           | 240 GB | 1       | 5     | 0     | 0.01   |
| HP        | SSD S700           | 120 GB | 1       | 0     | 0     | 0.00   |
