Corsair NVMe Drives
===================

This is a list of all tested Corsair NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Corsair   | Force MP600        | 2 TB   | 2       | 336   | 0     | 0.92   |
| Corsair   | Force MP510        | 480 GB | 2       | 224   | 0     | 0.62   |
| Corsair   | Force MP510        | 240 GB | 4       | 209   | 0     | 0.57   |
| Corsair   | Force MP600        | 500 GB | 2       | 195   | 0     | 0.53   |
| Corsair   | Force MP300        | 120 GB | 1       | 173   | 0     | 0.47   |
| Corsair   | Force MP600        | 1 TB   | 1       | 151   | 0     | 0.41   |
| Corsair   | Force MP510 1.9TB  | 1.9 TB | 1       | 109   | 0     | 0.30   |
| Corsair   | MP600 CORE         | 2 TB   | 1       | 73    | 0     | 0.20   |
| Corsair   | MP600 GS           | 1 TB   | 1       | 0     | 0     | 0.00   |
