Intenso Solid State Drives
==========================

This is a list of all tested Intenso solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Intenso   | SSD Sata III       | 120 GB | 6       | 499   | 0     | 1.37   |
| Intenso   | lntenso SSD Sat... | 120 GB | 1       | 469   | 0     | 1.29   |
| Intenso   | SSD SATAIII        | 120 GB | 6       | 379   | 1     | 1.04   |
| Intenso   | JAJMS600M128G      | 128 GB | 1       | 245   | 0     | 0.67   |
| Intenso   | SSD                | 128 GB | 16      | 187   | 0     | 0.51   |
| Intenso   | JAJMS600M256G      | 256 GB | 3       | 167   | 0     | 0.46   |
| Intenso   | IONN SSD           | 256 GB | 3       | 149   | 0     | 0.41   |
| Intenso   | SSD Sata III       | 250 GB | 2       | 138   | 0     | 0.38   |
| Intenso   | SSD                | 256 GB | 2       | 125   | 0     | 0.34   |
| Intenso   | SSD Sata III       | 256 GB | 4       | 76    | 0     | 0.21   |
| Intenso   | SSD                | 120 GB | 6       | 76    | 0     | 0.21   |
| Intenso   | SATA III SSD       | 480 GB | 2       | 72    | 0     | 0.20   |
| Intenso   | JAJM600M256C       | 256 GB | 1       | 70    | 0     | 0.19   |
| Intenso   | SSD Sata III       | 128 GB | 6       | 56    | 9     | 0.16   |
| Intenso   | JAJMS600M512G      | 512 GB | 1       | 56    | 0     | 0.15   |
| Intenso   | SATA3 240GB SSD    | 240 GB | 1       | 35    | 0     | 0.10   |
| Intenso   | SSD Sata III       | 240 GB | 1       | 10    | 0     | 0.03   |
| Intenso   | SSDAS256           | 256 GB | 1       | 0     | 0     | 0.00   |
| Intenso   | JAJMS600M1TB       | 1 TB   | 1       | 0     | 0     | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Intenso   | Unknown                | 15     | 42      | 195   | 2     | 0.54   |
| Intenso   | Phison Driven OEM SSDs | 2      | 18      | 174   | 0     | 0.48   |
| Intenso   | Silicon Motion base... | 2      | 4       | 132   | 0     | 0.36   |
