SPCC Solid State Drives
=======================

This is a list of all tested SPCC solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| SPCC      | SSD                | 64 GB  | 5       | 546   | 0     | 1.50   |
| SPCC      | SSD                | 120 GB | 9       | 483   | 0     | 1.32   |
| SPCC      | SSD                | 1 TB   | 21      | 456   | 0     | 1.25   |
| SPCC      | M.2 SSD            | 128 GB | 3       | 217   | 0     | 0.60   |
| SPCC      | SSD                | 240 GB | 2       | 216   | 0     | 0.59   |
| SPCC      | SPCCSolidStateDisk | 256 GB | 3       | 144   | 0     | 0.40   |
| SPCC      | SSD                | 128 GB | 24      | 121   | 1     | 0.32   |
| SPCC      | SSD                | 512 GB | 9       | 112   | 0     | 0.31   |
| SPCC      | SSD                | 256 GB | 18      | 101   | 1     | 0.27   |
| SPCC      | M.2 SSD            | 256 GB | 1       | 178   | 2     | 0.16   |
| SPCC      | SSD                | 55 GB  | 1       | 18    | 0     | 0.05   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| SPCC      | Phison Driven OEM SSDs | 7      | 88      | 259   | 1     | 0.71   |
| SPCC      | Unknown                | 4      | 8       | 160   | 1     | 0.40   |
