KingSpec Solid State Drives
===========================

This is a list of all tested KingSpec solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| KingSpec  | NT-64              | 64 GB  | 1       | 1033  | 0     | 2.83   |
| KingSpec  | NT-32              | 32 GB  | 2       | 690   | 0     | 1.89   |
| KingSpec  | KSD-SA25.7-016MJ   | 16 GB  | 1       | 648   | 0     | 1.78   |
| KingSpec  | P3-120             | 120 GB | 1       | 385   | 0     | 1.06   |
| KingSpec  | P4-120             | 120 GB | 3       | 265   | 0     | 0.73   |
| KingSpec  | MT-64              | 64 GB  | 2       | 225   | 0     | 0.62   |
| KingSpec  | NT-128             | 128 GB | 3       | 148   | 0     | 0.41   |
| KingSpec  | Q-720              | 720 GB | 2       | 140   | 0     | 0.38   |
| KingSpec  | ACSC2M064mSA       | 64 GB  | 1       | 125   | 0     | 0.34   |
| KingSpec  | MT-1TB             | 1 TB   | 1       | 118   | 0     | 0.33   |
| KingSpec  | MT-128             | 128 GB | 6       | 93    | 0     | 0.26   |
| KingSpec  | NT-512             | 512 GB | 4       | 73    | 0     | 0.20   |
| KingSpec  | MT-256             | 256 GB | 1       | 47    | 0     | 0.13   |
| KingSpec  | P3-128             | 128 GB | 2       | 117   | 3     | 0.13   |
| KingSpec  | P3-256             | 256 GB | 1       | 35    | 0     | 0.10   |
| KingSpec  | NT-256             | 256 GB | 4       | 33    | 0     | 0.09   |
| KingSpec  | P4-960             | 960 GB | 1       | 15    | 0     | 0.04   |
| KingSpec  | KSD-SA25.7-008MJ   | 8 GB   | 1       | 4     | 0     | 0.01   |
| KingSpec  | P3-512-TM          | 512 GB | 1       | 1     | 0     | 0.00   |
| KingSpec  | P3-1TB             | 1 TB   | 1       | 1     | 0     | 0.00   |
| KingSpec  | KDM-SA.51-008GMJ   | 8 GB   | 1       | 0     | 0     | 0.00   |
| KingSpec  | P3-512             | 512 GB | 1       | 251   | 1014  | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| KingSpec  | Unknown                | 17     | 28      | 190   | 37    | 0.48   |
| KingSpec  | JMicron/Maxiotek ba... | 5      | 13      | 146   | 0     | 0.40   |
