Phison Solid State Drives
=========================

This is a list of all tested Phison solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Phison    | SATA SSD           | 120 GB | 4       | 741   | 0     | 2.03   |
| Phison    | BP4 mSATA SSD      | 240 GB | 1       | 688   | 0     | 1.89   |
| Phison    | SATA SSD           | 16 GB  | 45      | 544   | 0     | 1.49   |
| Phison    | SATA SSD           | 8 GB   | 1       | 508   | 0     | 1.39   |
| Phison    | SATA SSD           | 128 GB | 5       | 438   | 0     | 1.20   |
| Phison    | SATA SSD           | 32 GB  | 7       | 301   | 0     | 0.83   |
| Phison    | SATA SSD           | 256 GB | 1       | 194   | 0     | 0.53   |
| Phison    | SATA SSD           | 1 TB   | 1       | 105   | 0     | 0.29   |
| Phison    | SATA SSD           | 64 GB  | 3       | 95    | 0     | 0.26   |
| Phison    | NETLIST SSD 8GB... | 8 GB   | 1       | 833   | 8     | 0.25   |
| Phison    | SATA SSD           | 240 GB | 1       | 35    | 0     | 0.10   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Phison    | Phison Driven SSDs     | 1      | 1       | 688   | 0     | 1.89   |
| Phison    | Driven OEM SSDs        | 8      | 67      | 487   | 0     | 1.34   |
| Phison    | Unknown                | 2      | 2       | 513   | 4     | 0.39   |
