Hoodisk Solid State Drives
==========================

This is a list of all tested Hoodisk solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Hoodisk   | SSD                | 16 GB  | 18      | 536   | 0     | 1.47   |
| Hoodisk   | SSD                | 32 GB  | 50      | 515   | 0     | 1.41   |
| Hoodisk   | SSD                | 128 GB | 48      | 413   | 0     | 1.13   |
| Hoodisk   | SSD                | 64 GB  | 51      | 413   | 0     | 1.13   |
| Hoodisk   | SSD                | 256 GB | 10      | 356   | 0     | 0.98   |
| Hoodisk   | SSD                | 512 GB | 3       | 353   | 0     | 0.97   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Hoodisk   | Phison Driven OEM SSDs | 5      | 177     | 451   | 0     | 1.24   |
| Hoodisk   | Unknown                | 1      | 3       | 353   | 0     | 0.97   |
