Seagate NVMe Drives
===================

This is a list of all tested Seagate NVMe drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

NVME by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Seagate   | IronWolf ZP500N... | 500 GB | 1       | 195   | 0     | 0.53   |
| Seagate   | FireCuda 520 SS... | 1 TB   | 1       | 111   | 0     | 0.30   |
| Seagate   | FireCuda 520 SS... | 500 GB | 6       | 103   | 0     | 0.28   |
| Seagate   | FireCuda 520 SS... | 2 TB   | 1       | 68    | 0     | 0.19   |
| Seagate   | BarraCuda Q5 ZP... | 500 GB | 2       | 53    | 0     | 0.15   |
| Seagate   | FireCuda 530 ZP... | 4 TB   | 1       | 35    | 0     | 0.10   |
| Seagate   | BarraCuda 510 S... | 512 GB | 1       | 29    | 0     | 0.08   |
| Seagate   | BarraCuda 510 S... | 250 GB | 1       | 14    | 0     | 0.04   |
| Seagate   | FireCuda 510 SS... | 500 GB | 1       | 1     | 0     | 0.00   |
| Seagate   | FireCuda 530 ZP... | 4 TB   | 1       | 1     | 0     | 0.00   |
