smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       BR 128GB
Serial Number:                      --
Firmware Version:                   V0728A
PCI Vendor ID:                      0x126f
PCI Vendor Subsystem ID:            0x2261
IEEE OUI Identifier:                0x5cd2e4
Total NVM Capacity:                 128,035,676,160 [128 GB]
Unallocated NVM Capacity:           0
Controller ID:                      1
NVMe Version:                       1.3
Number of Namespaces:               1
Namespace 1 Size/Capacity:          128,035,676,160 [128 GB]
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            efcdab ...
Local Time is:                      Thu Jan 12 17:59:39 2023 UTC
Firmware Updates (0x14):            2 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x005f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat Timestmp
Log Page Attributes (0x07):         S/H_per_NS Cmd_Eff_Lg Ext_Get_Lg
Maximum Data Transfer Size:         64 Pages
Warning  Comp. Temp. Threshold:     83 Celsius
Critical Comp. Temp. Threshold:     85 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     9.00W       -        -    0  0  0  0        0       0

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        40 Celsius
Available Spare:                    100%
Available Spare Threshold:          13%
Percentage Used:                    0%
Data Units Read:                    960,893 [491 GB]
Data Units Written:                 560,036 [286 GB]
Host Read Commands:                 9,271,209
Host Write Commands:                8,201,448
Controller Busy Time:               43
Power Cycles:                       114
Power On Hours:                     39
Unsafe Shutdowns:                   41
Media and Data Integrity Errors:    0
Error Information Log Entries:      0
Warning  Comp. Temperature Time:    1
Critical Comp. Temperature Time:    0
Temperature Sensor 1:               -37 Celsius
Thermal Temp. 1 Transition Count:   218
Thermal Temp. 2 Transition Count:   51
Thermal Temp. 1 Total Time:         5368417
Thermal Temp. 2 Total Time:         4975

Error Information (NVMe Log 0x01, 16 of 256 entries)
No Errors Logged

