SATADOM Solid State Drives
==========================

This is a list of all tested SATADOM solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| SATADOM   | ML 3SE             | 64 GB  | 1       | 470   | 0     | 1.29   |
| SATADOM   | SL 3IE3 V2         | 64 GB  | 7       | 185   | 0     | 0.51   |
| SATADOM   | SH 3ME4            | 16 GB  | 1       | 31    | 0     | 0.09   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| SATADOM   | Unknown                | 1      | 1       | 470   | 0     | 1.29   |
| SATADOM   | Innodisk 3IE3/3ME3/... | 1      | 7       | 185   | 0     | 0.51   |
| SATADOM   | Innodisk 1IE3/3IE3/... | 1      | 1       | 31    | 0     | 0.09   |
