Apacer Solid State Drives
=========================

This is a list of all tested Apacer solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Apacer    | AST220             | 120 GB | 1       | 610   | 0     | 1.67   |
| Apacer    | AS510S             | 128 GB | 1       | 592   | 0     | 1.62   |
| Apacer    | AS220              | 64 GB  | 1       | 536   | 0     | 1.47   |
| Apacer    | 32GB SATA Flash... | 32 GB  | 10      | 645   | 105   | 1.30   |
| Apacer    | 128GB SATA Flas... | 128 GB | 3       | 396   | 0     | 1.09   |
| Apacer    | APSDM050GM1AN-T... | 54 GB  | 1       | 364   | 0     | 1.00   |
| Apacer    | 64GB SATA Flash... | 64 GB  | 10      | 385   | 20    | 0.94   |
| Apacer    | 16GB SATA Flash... | 16 GB  | 19      | 471   | 13    | 0.89   |
| Apacer    | AS350              | 120 GB | 1       | 274   | 0     | 0.75   |
| Apacer    | AS340              | 240 GB | 5       | 209   | 0     | 0.57   |
| Apacer    | AS450              | 240 GB | 1       | 123   | 0     | 0.34   |
| Apacer    | AS330              | 240 GB | 1       | 1006  | 8     | 0.31   |
| Apacer    | AS350              | 256 GB | 4       | 104   | 0     | 0.29   |
| Apacer    | AS350              | 128 GB | 4       | 100   | 0     | 0.28   |
| Apacer    | APM050GMFAN-4MTM1  | 54 GB  | 1       | 84    | 0     | 0.23   |
| Apacer    | 8GB SATA Flash ... | 8 GB   | 2       | 846   | 29    | 0.15   |
| Apacer    | AS340              | 120 GB | 1       | 25    | 0     | 0.07   |
| Apacer    | 256GB SATA Flas... | 256 GB | 1       | 17    | 0     | 0.05   |
| Apacer    | 4GB SATA Flash ... | 4 GB   | 1       | 14    | 0     | 0.04   |
| Apacer    | AS681              | 240 GB | 1       | 14    | 0     | 0.04   |
| Apacer    | AS220              | 256 GB | 1       | 3     | 0     | 0.01   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Apacer    | SSDs                   | 3      | 14      | 547   | 75    | 1.16   |
| Apacer    | SDM4 Series SSD Module | 2      | 29      | 441   | 16    | 0.90   |
| Apacer    | Unknown                | 12     | 18      | 246   | 1     | 0.54   |
| Apacer    | AS340 SSDs             | 2      | 6       | 179   | 0     | 0.49   |
| Apacer    | SDM5/5A/5A-M Series... | 2      | 3       | 569   | 20    | 0.11   |
