#
# For a description of the syntax of this configuration file,
# see scripts/kbuild/config-language.txt.
#

menu "Networking Utilities"

config FEATURE_IPV6
	bool "Enable IPv6 support"
	default y
	help
	  Enable IPv6 support in busybox.
	  This adds IPv6 support in the networking applets.

config FEATURE_UNIX_LOCAL
	bool "Enable Unix domain socket support (usually not needed)"
	default n
	help
	  Enable Unix domain socket support in all busybox networking
	  applets.  Address of the form local:/path/to/unix/socket
	  will be recognized.

	  This extension is almost never used in real world usage.
	  You most likely want to say N.

config FEATURE_PREFER_IPV4_ADDRESS
	bool "Prefer IPv4 addresses from DNS queries"
	default y
	depends on FEATURE_IPV6
	help
	  Use IPv4 address of network host if it has one.

	  If this option is off, the first returned address will be used.
	  This may cause problems when your DNS server is IPv6-capable and
	  is returning IPv6 host addresses too. If IPv6 address
	  precedes IPv4 one in DNS reply, busybox network applets
	  (e.g. wget) will use IPv6 address. On an IPv6-incapable host
	  or network applets will fail to connect to the host
	  using IPv6 address.

config VERBOSE_RESOLUTION_ERRORS
	bool "Verbose resolution errors"
	default n
	help
	  Enable if you are not satisfied with simplistic
	  "can't resolve 'hostname.com'" and want to know more.
	  This may increase size of your executable a bit.

INSERT

source networking/udhcp/Config.in

config IFUPDOWN_UDHCPC_CMD_OPTIONS
	string "ifup udhcpc command line options"
	default "-R -n"
	depends on IFUPDOWN && UDHCPC
	help
	  Command line options to pass to udhcpc from ifup.
	  Intended to alter options not available in /etc/network/interfaces.
	  (IE: --syslog --background etc...)

endmenu
